

**8200**

**CHANGING STATION**

IMPORTANT. RETAIN FOR FUTURE REFERENCE. READ CAREFULLY.

**COMPLIES WITH BS EN 12221-1 2008 + A1:2013**

**Assembly Instructions.**

The stairs can be positioned on the left hand or the right hand side of the unit. Refer to these instructions before assembly and where necessary refer to the component List at the back.

**Adults Required For Assembly**.



**Additional Tools Required**.



**Maintenance.**

Examine all fasteners periodically and retighten where necessary.

Care must be taken not to over tighten the fasteners.

Some residual dust from the manufacturing process may be apparent.

Your unit may be cleaned with a damp cloth.

Stubborn marks may be removed with a mild detergent or

non-abrasive cream cleaner.

**WARNING: “DO NOT LEAVE A CHILD UNATTENDED”**

Be aware of the risk of open fires and other sources of strong heat such as electric bar fires, gas fires, etc. in the near vicinity of the changing unit.

Do not use the changing unit when any part is broken torn or missing.

Any additional or replacement parts shall only be obtained from the manufacturer or distributor.

Maximum size cot mattress 120cm x 60cm (not included)

Intended for use for children from birth to 21kg.

This unit is designed for use indoors on a flat level surface.

Manufactured by:

Mike Miller Associates Ltd.,

Syke Road, Wigton. Cumbria CA7 9NS

Tel: 016973 49774/45300 Fax: 016973 45511

Email: info@twoey.co.uk

Website: www.twoeytoys.com

Registered in England No: 1425839

Registered Office: The Old Brewery, Caldbeck.

Cumbria CA7 8EW































`





